Transport priority

Integer value used to attach a priority to data passed through the DDS. This can be used to implement priority bands that ensure high priority data is more valuable within the DDS than lower priority data. Source: OpenSplice Glossary