ISO/IEC 7816-10 Identification cards — Integrated circuit(s) cards with contacts — Part 10: Electronic signals and answer to reset for synchronous cards

return to the ISO Standards

Data sheet for Identification cards — Integrated circuit(s) cards with contacts — Part 10: Electronic signals and answer to reset for synchronous cards

Title	Identification cards — Integrated circuit(s) cards with contacts — Part 10: Electronic signals and answer to reset for synchronous cards
Acronym
Version	1999
Document Number	7816-10
Release Date	1999
Reference	https://www.iso.org/obp/ui/#iso:std:iso-iec:7816:-10:ed-1:v2:en

Note: The following is an excerpt from the official ISO catalog. It is provided here as a convenience and is not authoritative. Refer to the original document as the authoritative reference.

Scope

This part of ISO/IEC 7816 specifies the power, signal structures, and the structure for the answer to reset between an integrated circuit(s) card with synchronous transmission and an interface device such as a terminal.

The specifications in ISO/IEC 7816-3 apply where appropriate unless otherwise stated here.

It also covers signal rates, operating conditions, and communication with the integrated circuit(s) card.

This part of ISO/IEC 7816 specifies two types of synchronous cards: type 1 and type 2.