Consolidate Generation

Return to Glossary

Consolidate Generation attempts to improve on the inefficiency of spot, by running distribution cables to multiple structures (such as tents). It improves the efficiency by better matching the load to the source. However, that optimization ends up being more complicated, as a result, it is not widely used.

Source: Consolidate Generation