Transport priority

Integer value used to attach a priority to data passed through the data_distribution_service_dds. This can be used to implement priority bands that ensure high priority data is more valuable within the DDS than lower priority data. Source: OpenSplice Glossary