Disconnected, Intermittent and Limited (DIL)

Return to Glossary

Disconnected, Intermittent and Limited (DIL) occur in wireless/mobile networking environments, e.g. rural area networks, vehicular networks, battlefield networks and other resource-constrained or disadvantaged networks. Efficient and effective interoperability in these networks is highly demanded for various mission-critical application scenarios such as disaster relief in ravaged regions, search and rescue in remote areas and military/tactical operations in hostile environments.

Source: https://icc2018.ieee-icc.org/workshop/3rd-international-workshop-service-oriented-computing-disconnected-intermittent-and-limited