Media Access Control (MAC)

Return to Glossary

Media Access Control (MAC) is a sublayer of the Data Link Layer (DLL) in the seven-layer Open Systems Interconnection (OSI) Model. MAC is responsible for the transmission of data packets to and from the Network Interface Card (NIC), and to and from another remotely shared channel.