ISO/IEC 7816-12 Identification cards - Integrated circuit cards — Part 12: Cards with contacts — USB electrical interface and operating procedures

return to the ISO Standards

Data sheet for Identification cards - Integrated circuit cards — Part 12: Cards with contacts — USB electrical interface and operating procedures

Title	Identification cards - Integrated circuit cards — Part 12: Cards with contacts — USB electrical interface and operating procedures
Acronym
Version	2005
Document Number	7816-12
Release Date	2005
Reference	https://www.iso.org/obp/ui/#iso:std:iso-iec:7816:-12:ed-1:v1:en

Note: The following is an excerpt from the official ISO catalog. It is provided here as a convenience and is not authoritative. Refer to the original document as the authoritative reference.

Scope

This part of ISO/IEC 7816 specifies the operating conditions of an integrated circuit card that provides a USB interface. Figure 1 shows the assignment of the contact fields for a USB interface and - to illustrate interoperability - the assignment as used in ISO/IEC 7816-03 Identification cards — Integrated circuit cards — Part 3: Cards with contacts — Electrical interface and transmission protocols.

<caption>Assignemnt of contacts for USB Integrated Circuit Card</cpation>